Device 1 options are:
Row 0 => Verify	,TRUERow 1 ===== General CPLD And PROM Properties =====,
Row 2 => Erase Before Programming	,TRUERow 3 => Read Protect	,FALSERow 4 => PROM/CoolRunner-II Usercode (8 Hex Digit)	,
Row 14 ===== PROM Specific Properties =====,
Row 15 => Load FPGA	,FALSERow 16 => Parallel Mode	,FALSE