set -tmpdir ../synth/__projnav
set -xsthdpdir ../synth/xst
run
-ifn ../synth/example_top.prj
-ifmt mixed
-ofn example_top
-ofmt NGC
-p xc6vlx130t-2-ff1156
-top example_top
-opt_mode Speed
-opt_level 1
-power NO
-iuc NO
-uc constraints.xcf
-lso ../synth/example_top.lso
-keep_hierarchy NO
-netlist_hierarchy as_optimized
-rtlview Yes
-glob_opt AllClockNets
-read_cores YES
-write_timing_constraints NO
-cross_clock_analysis NO
-hierarchy_separator /
-bus_delimiter <>
-case maintain
-slice_utilization_ratio 100
-bram_utilization_ratio 100
-dsp_utilization_ratio 100
-lc auto
-reduce_control_sets auto
-fsm_extract YES -fsm_encoding Auto
-safe_implementation No
-fsm_style lut
-ram_extract Yes
-ram_style Auto
-rom_extract Yes
-shreg_extract YES
-rom_style Auto
-auto_bram_packing NO
-resource_sharing YES
-async_to_sync NO
-use_dsp48 auto
-iobuf YES
-bufg 32
-register_duplication YES
-register_balancing No
-optimize_primitives NO
-use_clock_enable Auto
-use_sync_set Auto
-use_sync_reset Auto
-iob auto
-equivalent_register_removal YES
-slice_utilization_ratio_maxmargin 5
quit
